Lobster Telescope

Effective Areas

  To obtain the flux in the relevant focus from a source, multiply the source

                    intensity by the effective area. For the background multiplying the

background brightness  by the effective area x (4/R

2
) gives the background

                                                                                                      rate per unit area at the detector.