Anticipated

Performance

0.1-0.5 keV  channel 0.5-3.5 keV  channel

                                    (flux indexed to  -  0.135-0.355 keV to 0.5-2.4 keV)

n et mean count rate from Crab

1
- 2.0 s

-1

measurement limit at S/N = 5               0.9 x 10

-12

2.1 x 10

-12

                   (1 day exposure)
erg cm

-2
 s

-1
erg cm

-2
 s

-1

                               (
0.15 mCrab )

detection limit at 5s significance          0.6 x 10

-12
1.0 x 10

-12

                (1 day exposure)
erg cm

-2
 s

-1
erg cm

-2
 s

-1

                               (
0.08 mCrab )

1
       Count rates derated by a factor of 0.77 from best estimates to allow for

unforeseen imperfections.